# Communication failure

Navigation: Valve Firmware > Interface > EtherCAT > # Communication failure |

Failure detection with CPA | Action
Network failure: No EtherCAT communication is active | -Check EtherCAT cable. -Check the EtherCAT connection to master. -Check the process data output watchdog – SyncManager2 settings

| If you need any further information, please contact one of our service centers. You will find the addresses on our website: www.vatgroup.com.