# Slave Status - Bitmap description

Navigation: Valve Firmware > Interface > Profibus > Cyclic Buffers > Input Buffer > # Slave Status - Bitmap description |

Slave Status
Bit | Name | Description
0 - 1 | Access Mode | 0 = Local 1 = Remote 2 = Remote Locked 3 = Local and Remote
2 | Freeze Mode | 0 = Not Frozen, 1 = Frozen
3 | Offline Status | 0 = Online, 1 = Offline
4 - 7 | Not Used | Reserved
8 | Service Request | 0 = Inactive, 1 = Active
9 | Compressed Air Failure | 0 = No Failure, 1 = Failure
10 | PFO Voltage Low | 0 = Voltage High Enough, 1 = Voltage Low
11 | Iso Valve Failure | 0 = No Failure, 1 = Failure
10 - 15 | Not Used | Reserved