# Adaptive Learn Data

Navigation: CPA > Pressure > # Adaptive Learn Data |

Adaptive Learn Data window supports different learn data functionality. It shows the saved actual pressure value on the specific learn position of each learn bank.

Per default the graph shows the current learn data information of the connected controller. Pressure unit of the y-axis can be adapted in the CPA Scaling.

Load from File

This function loads the learn bank information and shows it in the graph. It's possible to load the learn data directly from a Diagnostic File as well as a single learn bank information generated by the Save to File option.

If a file content is loaded then the Filename shows the file path.

Save to File

Learn Data information which is showed in the graph will be exported. This file can be loaded later again with the Load from File option in case of the file format is not changed.

Load from Valve

Chart data information will be updated with the connected controller learn data. This options is required if previously the Load from File option is executed and now the connected controller learn data should be displayed again.

Save to Valve

Transfer a single learn bank loaded from a file or from the connected controller to a defined learn bank on the controller. Be aware that the original learn data bank information on the connected controller are lost afterward. In case of a recovery options is desired then execute the Save to File option in advance.

Transferring Learn Data

•If no learn data information are available then either execute a learn procedure see Adaptive Learn or use the Load from File.

•Execute Save to File option with the default csv file format.

•Connect different controller where the learn data needs to be transferred. Open Adaptive Learn Data window and execute Load from File. Select the File which was created by the Save to File option one step before.

•Execute Save to Valve as last step.