# Input Buffer

Navigation: Valve Firmware > Interface > CC-Link > Cyclic Communication - Process Data > # Input Buffer |

Input Buffer
Byte | Word | Parameter | Content | Bytes | Words
0 | 0 | 1 | Pressure | 4 | 2
1
2 | 1
3
4 | 2 | 2 | Pressure Sensor 1 | 4 | 2
5
6 | 3
7
8 | 4 | 3 | Pressure Sensor 2 | 4 | 2
9
10 | 5
11
12 | 6 | 4 | Position | 4 | 2
13
14 | 7
15
16 | 8 | 5 | Target Position | 4 | 2
17
18 | 9
19
20 | 10 | 6 | Control Mode | 1 | 1
21 |  | Padding Byte | 1
22 | 11 | 7 | Fatal Error | 2 | 1
23
24 | 12 | 8 | PKW | 2 | 1
25
26 | 13 | 9 | PKW | 2 | 1
27
28 | 14 | 10 | PKW | 2 | 1
29
30 | 15 | 11 | PKW | 2 | 1
31
32 | 16 | 12 | General Status | 2 | 1
33
34 | 17 | 13 | General Warnings | 2 | 1
35
36 | 18 | 14 | Extended Warnings | 2 | 1
37
38 | 19 | 15 | Cluster Monitoring Address | 1 | 1
39 |  |  | Padding Byte | 1
40 | 16 | 16 | Cluster Valve Position | 4 | 2
41
42 | 17
43
44 | 18 | 17 | Cluster Valve Control Mode | 1 | 1
45 |  | Padding Byte | 1
46 | 19 | 14 | Cluster Valve Status | 2 | 1
47
48 | 20 | 15 | Cluster Valve Warnings | 2 | 1

Bitmap parameter definitions:

General status | 0 | Fieldbus Data Valid
General status | 1 | Zero Executed
General status | 2 | Ping Pong RX
General status | 3 | Pressure Simulation
General Status | 4 | Pressure Setpoint Reached
General Status | 5,6 | Not Used
General Status | 7 | Access Mode
General Status | 8 | Access Mode
General Status | 9 | Warnings Active
General Status | 10 | Sealed
General Status | 11...15 | Not Used

General Warnings | 0 | Service Request
General Warnings | 1 | Learn Data Set
General Warnings | 2 | Compressed Air Failure
General Warnings | 3 | Power Failure Battery
General Warnings | 4 | Sensor Overlapping
General Warnings | 5 | Iso Valve Failure
General Warnings | 6 | Offline
General Warnings | 7…9 | Not Used
General Warnings | 10 | Sensor Measurement Unit Faulty, Plasma On
General Warnings | 11…15 | Not Used

Extended Warnings | 0 | Remote Control Not Possible
Extended Warnings | 1 | Actual Control Mode Setpoint Not Allowed
Extended Warnings | 2 | Zero Disabled
Extended Warnings | 3 | PFO Deactivated
Extended Warnings | 4 | Not Used
Extended Warnings | 5 | Out Of Range Pressure Setpoint
Extended Warnings | 6 | Out Of Range Position Setpoint
Extended Warnings | 7 | Not Used
Extended Warnings | 8 | Out Of Range Sensor 1
Extended Warnings | 9 | Out Of Range Sensor 2
Extended Warnings | 10 | Out Of Range Control Mode Setpoint
Extended Warnings | 11 | Out Of Range Control Setpoint
Extended Warnings | 12 | Process Data Settings not valid
Extended Warnings | 13…15 | Not Used

Cluster Valve Control Setpoint | 0 | Freeze
Cluster Valve Control Setpoint | 1 | Freeze Mode: 0 Position, 1 Close
Cluster Valve Control Setpoint | 2 | Data Valid
Cluster Valve Control Setpoint | 3…15 | Reserved

Cluster Valve Status | 0…1 | Access Mode
Cluster Valve Status | 2 | Freeze Mode
Cluster Valve Status | 3 | Offline Status
Cluster Valve Status | 4…7 | Reserved
Cluster Valve Status | 8 | Service Request
Cluster Valve Status | 9 | Compressed Air Failure
Cluster Valve Status | 10 | PFO Voltage Low
Cluster Valve Status | 11 | Iso Valve Failure
Cluster Valve Status | 10…15 | Reserved

Cluster Valve Warning | 0 | Out of Range Freeze Position Setpoint
Cluster Valve Warning | 1 | Out of Range Freeze Address Setpoint
Cluster Valve Warning | 2 | Out Of Range Control Setpoint
Cluster Valve Warning | 3 | Out of Range Monitoring Address Setpoint
Cluster Valve Warning | 4…15 | Reserved