# Device identification, Rotary switches

Navigation: Valve Firmware > Interface > EtherCAT > # Device identification, Rotary switches |

The Device Identification value (ID) is set by three hexadecimal rotary switches. That means the supported address range is 0-0xFFF in hexadecimal or 0-4095 in decimal.

| The Device Identification value is read once after power on.

Example: 0

Note: In IC2 both kind of addresses Requested ID and Station Alias is defined by rotary switches.