# Set Position Offset via RS232

Navigation: »No topics above this level« # Set Position Offset via RS232 |

It is also possible to set a Position Offset over an Interface RS232 command.

With the command:

c:74abbbbb[CR][LF] à a = sign; b = offset (range: -30000 to 30000).

If the c:74abbbbb command is send to the Valve the Position Adaption Enable will Automatically be active.

To get the Actual Position Offset from the Valve, the user can send the following Get-Command:

i:74 à Response will be i:74abbbbb à ab = Position Offset: -30000 to 30000.

Like in the example before with a Position Offset = 5 à the Response will be: i:74005000[CR][LF]