# Control Parameter

Navigation: Valve Firmware > Pressure Control > Adaptive algorithm > # Control Parameter |

Parameter | Description
Gain Factor | Main parameter to adapt the performance of the pressure control algorithm. A higher gain results in a faster response, higher over- / undershoots of pressure. A lower gain results in slower response, lower over- / undershoot of pressure.
Sensor Delay | For compensation of delays during the pressure detection. Pipes and orifices for sensor attachment can cause delays in response time and could impact badly the pressure control stability. By adapting this parameter to the approximate delay time stability problems can be reduced. But control response time will be slowed down by this measure.
Learn Data Selection | There are up to 4 different learn data sets available. Select which Learn Data set the adaptive controller shall use for pressure control.