# Power up

Navigation: Valve Firmware > Display information > # Power up |

Description | Digit 1 | Digit 2 | Digit 3 | Digit 4
● 1 st Power On: All dots are illuminated | # | # | # | #
● 2 nd Valve series e.g. 67.0 |  | 6 | 7 | 0
● 3 rd Firmware: generation.type e.g. 01.0C | 0 | 1 | 0 | C
● 4 th Firmware: version.firmware e.g. 07.00 | 0 | 7 | 0 | 0
● 5 th Controller configuration: e.g. 11.00 | Controller 1=H1 2=H2 3=H3 4=H4 5=H5 6=H6 7=H7 | Interface 1=RS232/RS485 2=EtherCAT 3=DeviceNet 5=Logic | Options 00=none 01=SPS 02=PFO 03=Cluster 04=SPS & PFO 05=SPS & Cluster 06=PFO & Cluster 07=SPS & PFO & Cluster
‘Ho’ homing is running | H | o |  |