# Connection Loss Reaction

Navigation: Valve Firmware > Interface > Profibus > Communication > # Connection Loss Reaction |

If the connection to the Profibus gets lost, the valve will go to desired state (open or close).
Enable = Activating of the feature
State = True if the the connection loss has been detected
Functionality = Position/Mode where the valve ends up upon the connection loss

Parameter location:

CPA
Interface Profibus.Connection Loss Reaction