# Link cable

Navigation: »No topics above this level« # Link cable |

RJ45 pinning: active pins 4 and 5

Pin | Description
1 | not used
2 | not used
3 | not used
4 | Data
5 | Data
6 | not used
7 | not used
8 | not used

VAT recommends a cable with the following specification:

•Standard patch cable

•Category 5 or higher

•Double ended with shielded RJ45 connector

•Straight through connection 1:1