# Station Number

Navigation: Valve Firmware > Interface > CC-Link > Configuration > # Station Number |

The parameter "Station number" is used to distinguish between stations on the CC-Link network. Unique station numbers in consecutive order without duplication must be used, when assigning stations to the CC-Link network. The allowed range is from 1 to 64. "Station number" can be set via CPA as it is shown on the snapshot: