# Mode

Navigation: Valve Firmware > Interface > DeviceNet > LEDs > # Mode |

State of operation

LED Color | Description
GREEN | Operating in Normal Condition
FLASHING GREEN | The device needs commissioning due to configuration missing, incomplete or incorrect. The Device may be in the Standby state.
FLASHING RED | Recoverable Fault
RED | The device has an unrecoverable fault may need replacing. •Bus Off •Queue overload •Duplicate MAC ID
FLASHING GREEN & RED | The Device is in Self Test.