# Extended cyclic setting

Navigation: Valve Firmware > Interface > CC-Link > Configuration > # Extended cyclic setting |

This is the extended cyclic transmission. The extended cyclic points can be set as 2 times, 4 times or 8 times of the normal cyclic transmission points. In case of VAT controllers, it is always paired with "Number of occupied station" in the following way.

Number of occupied stations: 1 & Extended cyclic setting: Octuple

Number of occupied stations: 4 & Extended cyclic setting: Double

The VAT slave supports only these two combinations of the CC-Link parameter settings.

It can be configured via CPA as it is shown on the snapshot: