# Parameter

Navigation: Valve Firmware > Interface > RS232/485 > Input/Output > Digital Inputs > # Parameter |

| Parameter | Description
Digital Input 1..2 | Enable | True means it is supported. False means it is not supported
State | True means it is active. False means it is not active.
Functionality | Each digital input can be assigned one of the functionality descript at the table Functionality.
Inverted | Inverted the functionality of the signal.