# Record fields description

Navigation: Valve Firmware > Interface > Profibus > Communication > I&M0 record > # Record fields description |

Table - Description of the I&M0 record fields

Field | Description
Manufacturer ID | Manufacturer ID of VAT Vakuumventile AG listed at www.profibus.com/IM/Man_ID_Table.xml
Order ID | Order ID of the device. This is the Order ID, or model number or SKU number of the device. It is assigned by the vendor and should be equal to customer readable markings on the device.
Serial Number | Controller Serial Number
Hardware Revision | Hardware revision of the device
Software Revision Prefix | Same value as in GSD file Part FAB.CD.EF.GH
Software Revision 1 | Part YY of the controller Firmware Version F01.XX.YY.ZZ
Software Revision 2 | Part ZZ of the controller Firmware Version F01.XX.YY.ZZ
Software Revision 3 | Mapped part XX of the controller Firmware Version F01.XX.YY.ZZ in following way: XX == 0B à ‘Software Revision 1’ = 0 XX == 0C à ‘Software Revision 2’ = 1 XX == 0T à ‘Software Revision 3’ = 2 XX == 0P à ‘Software Revision 4’ = 3 XX == something else à ‘Software Revision 4’ = 9
Revision Counter | Initial value 0. Increments on every set of I&M data.
Profile ID | For details refer to\nwww.profibus.com/IM/Profile_ID_Table.xml
Profile Specific Type | For details refer to\nwww.profibus.com/IM/Profile_specific_type_table_6282.xml
Version | I&M version the Hilscher Stack
Supported | Bitmask that defines which I&M fields are supported by the device For details refer to Hilscher API manual PROFIBUS DP Slave Protocol API 19 EN.pdf chapter PROFIBUS_FSPMS_CMD_SET_IM0_REQ