# TCP/IP Settings

Navigation: Valve Firmware > Interface > EtherNet > # TCP/IP Settings |

Location: Parameters / Interface Ethernet / Settings

Parameter | Default Value | Description
--- | --- | ---
IP Address | 192.168.9.208 | Defines the address of the valve in the network Used if DHCP is off.
Subnet Mask | 255.255.255.0 | In IPv4 networks, it specifies how many bits make up the network prefix for an IP address. Together with the IP address, it defines the address of a device in the network. The network prefix part shows which devices are in a network.
Gateway | 192.168.9.111 | Address of the gateway. A gateway serves as a link between two systems or networks that use different protocols and communication services.
DHCP | OFF | The IPs address is automatically assigned by a DHCP server.
Telnet Port 1 | 503 | Communication port, range 501 ... 2500
Telnet Port 2 | 504 | Streaming port, range 501 ... 2500