# Range of Pressure and Position values

Navigation: Valve Firmware > Interface > CC-Link > Configuration > # Range of Pressure and Position values |

The range of all listed pressure and position values can be adjusted. That means, for example, that the valve position values for “CLOSE” and “OPEN” can be set to other ones then the default values 0 and 100’000.

|  | Default range limits
# | Parameter name | Min | Max
Inputs
1 | Pressure | 0 | 1’000´000
2 | Pressure Sensor 1 | 0 | 1’000’000
3 | Pressure Sensor 2 | 0 | 1’000’000
4 | Position | 0 | 100’000
5 | Target Position | 0 | 100’000
6 | Cluster Valve Position | 0 | 100’000
Outputs |
7 | Pressure Setpoint | 0 | 1’000’000
8 | Position Setpoint | 0 | 100’000
9 | Pressure Alignment Setpoint | 0 | 1’000’000
10 | External Digital Pressure Sensor 1 | 0 | 1’000’000
11 | External Digital Pressure Sensor 2 | 0 | 1’000’000
12 | Cluster Valve Freeze Position Setpoint | 0 | 100’000

The range of pressure and position values can be configured via CPA for each of the 12 parameters separately:

The range of pressure and position values is independent of the data type (signed integer and floating point). The internal accuracy of valve is for all positions is the precision of IEEE-754 Floating point number. If the range of pressure and position values is rising, the accuracy of pressure and position does not rise. This is only scaling that doesn't improve internal accuracy of values.