# Chart

Navigation: CPA > Main Window > # Chart |

The Chart allows to record any available parameter (max 10, 5 per axis). This can be defined within the Chart Content.

Right Click Menu

•Chart Content

•Scroll: Steady advance of the data display.

•Settings

Plots Axis 1, Plots Axis 2

•Option to hide parameter signal in the chart (if disabled this parameter is still recorded)

Record

•Start and stop of the recording.

•For more information see Record.

Clear

•Delete the actual chart data

•An active record is not interrupted by clear chart

Stop

•Stop the actual chart data

•Stop button change the function to "Start"

•An active record is not interrupted by when stopping the live chart.

Analyze

•Opens the Chart Analyzer with the current chart data for deeper analyze.

•For more information see Chart Analyzer.

Scan Rate

•right click on "Scan Rate" at the right bottom corner and select the desired scan rate.

•No limit, means as fast as it is possible over USB.