# Station address

Navigation: Valve Firmware > Interface > Profibus > Communication > # Station address |

Profibus Station Address has range from 0 to 126 but zero is reserved for diagnosis devices. Therefore the selected address needs to be in range 1..126.
Addresses are checked for duplicates. Master should have the lowest address 1, and slaves should follow starting with 2. This is only a recommendation: 1 is still allowed for a slave.