# Output Buffer

Navigation: Valve Firmware > Interface > CC-Link > Cyclic Communication - Process Data > # Output Buffer |

Output Buffer
Byte | Word | Parameter | Content | Bytes | Words
0 | 0 | 1 | Pressure Setpoint | 4 | 2
1
2 | 1
3
4 | 2 | 2 | Position Setpoint | 4 | 2
5
6 | 3
7
8 | 4 | 3 | Pressure Alignment | 4 | 2
9
10 | 5
11
12 | 6 | 4 | External Digital Pressure Sensor 1 | 4 | 2
13
14 | 7
15
16 | 8 | 5 | External Digital Pressure Sensor 2 | 4 | 2
17
18 | 9
19
20 | 10 | 6 | Control Mode Setpoint | 1 | 1
21 |  | Padding | 1
22 | 11 | 7 | General Control Setpoint | 2 | 1
23
24 | 12 | 8 | PKW | 2 | 1
25
26 | 13 | 9 | PKW | 2 | 1
27
28 | 14 | 10 | PKW | 2 | 1
29
30 | 15 | 11 | PKW | 2 | 1
31
32 | 16 | 12 | Cluster Freeze Position | 4 | 2
33
34 | 17
35
36 | 18 | 13 | Cluster Address | 1 | 1
37 |  | Padding | 1
38 | 19 | 14 | Cluster Valve Control Setpoint | 2 | 1
39
40 | 20 | 15 | Cluster Monitoring Address | 1 | 1
41 |  | Padding | 1

Bitmap parameter definitions:

Object | Bit | Parameter
General control setpoint | 0 | Zero
General control setpoint | 1 | Not Used
General control setpoint | 2 | Ping Pong TX
General control setpoint | 3 | Not Used
General control setpoint | 4 | Access Mode
General control setpoint | 5 | Plasma Mode On
General control setpoint | 6 | Plasma Mode Off
General control setpoint | 5…15 | Not Used