# Data Type of Pressure and Position values

Navigation: Valve Firmware > Interface > CC-Link > Configuration > # Data Type of Pressure and Position values |

The data type of different pressure and position values can be optionally changed between 32-bit signed integer and 32-bit floating point (IEEE-754 standard).

They are all set to the floating point type by default. The data type can be set via CPA for each of the 12 parameters separately: