# Connection Loss Reaction

Navigation: Valve Firmware > Interface > DeviceNet > Communication > # Connection Loss Reaction |

Connection Loss reaction defines what the valve is doing in case the DeviceNet connection get lost.

Parameter | Description
Enable | True enables the connection loss reaction, in case of False there is no reaction on a connection loss (compatible IC1 Setting keep Position)
State | Current connection loss state
Functionality | Defines the functionality in case of connection loss. This can be open or close.