# Digital Outputs

Navigation: Valve Firmware > Power connector IO > # Digital Outputs |

| Parameter | Description
Digital Output 1..2 | Enable | True means it is supported. False means it is not supported
State | True means it is active. False means it is not active.
Functionality | Open Indicate the Open status of the Valve. Close Indicate the Close status of the Valve. Hold Indicate the Hold status of the Valve.
Inverted | Inverted the functionality of the signal.