# Digital Inputs

Navigation: Valve Firmware > Power connector IO > # Digital Inputs |

| Parameter | Description
Digital Input 1.2 | Enable | True means it is supported. False means it is not supported
State | True means it is active. False means it is not active.
Functionality | Interlock Open Open the Valve. Interlock Close Close the Valve. Hold Hold the actual position. High priority functionality
Inverted | Inverted the functionality of the signal.