# Read from Device

Navigation: CPA > Tools > Configuration Tool > # Read from Device |

With the Read from Device Tool a image of the selected controller is created.

Devices:

Select the connected controller from where the image should be created. If there is only one controller connected the devices field is not visible at all - the image is created from the connected controller. Some informations like the Firmware Version, Valve Series and the Interface Type are also added as information to this file.

Device Info:

Show the Firmware Version, Valve Series and Interface Type of the selected controller. The file name is also set after the "Read from Device" button is pressed and the path and filename are set.

Options:

Select if the device settings and/or interface settings should be copied to the image.

Read from Device:

After clicking the button, enter the path and filename where the image should be stored. When clicking on save a progress bar appears within the configuration tool. Wait for the operation to finish - approx. 1 minute - status bar is then reporting either success or failure.