# Parameters

Navigation: »No topics above this level« # Parameters |

This menu shows all customer settings. Useful settings are described in the list bellow. Save a settings is possible to press save or enter key. Valve has to be in local mode.

Example: Set Restore Factory Parameters (see function description in list bellow)

* character after the parameter name means that this value has not yet been saved.

Parameter function list

Parameter name | Full Parameter name | Description
--- | --- | ---
Restore Factory Parameters | System.Services.Store/Restore Settings.Restore Factory Parameters | Set Valve back to factory state
Store User Parameters | System.Services.Store/Restore Settings.Store User Parameters | Store all non volatile parameter settings
Restore User Parameters | System.Services.Store/Restore Settings.Restore User Parameters | Restore all non volatile parameter settings. It is important that a store user parameter function has been executed in the past.
Configuration Lock Mode | System.Services.Configuration Lock Mode | If configuration lock mode is enabled, all non volatile parameter are not settable anymore.
Store Control Parameter Volatile | Pressure Control.General Settings.Store Control Parameter Volatile | If store control parameter volatile is set, no parameter setting will save in memory. That means, after loosing power (also a restart command), the old setting will be active.
Error Recovery | System.Service.ErrorRecovery | If Error Recovery is active, the error can be solved without a Restart and in this case without losing connection on the Interface(e.g. Ethercat Interface)

Copy to Clipboard with right click in values window

With this feature all parameters are copy to clipboard which are on the right side under values. For example to copy learn data of bank 1 in excel.