# Settings

Navigation: CPA > Main Window > Chart > # Settings |

Axis Settings

Axes range: every axis range (Axis 1, Axis 2) can be defined individually

Autoscale → the Chart will automatically adapt the scaling depending on the recorded data.

Manual scaling → the User can set min and max values for individual axis

Log scale → the Chart will show the axis in logarithmic format

Time Range

Chart defines the maximum duration of the showed data in the main window chart.

Record defines the duration of the recording. 1 hours means that only the last hour of the measurement is saved.

Chart Colors

In the field chart colors, it is possible to change the chart color of individual parameters(Auto save). Red Box are Parameters on Axis 1, Blue Box are Parameters on Axis 2.

Since the CPA v4.3.0

Only the used signals are visible. New structure of chart colors definition so that Parameter 2 color defines the second signal of the Axis 1 and the Parameter 6 color defines the first signal of Axis 2. Before Parameter 1 defines signal 1 and Parameter 2 defines second defined signal etc.