# Automated Controller

Navigation: Valve Firmware > Pressure Control > General Settings > # Automated Controller |

Define different Control Settings for different pressure ranges or for up - and down control.

With the 4 Controllers it is possible to define different pressure control settings.

The Automated Controller Selector can select one of the 4 Controllers depending on (either or)

•Target Pressure (Mode: Threshold)

•Up- or Down Control (Mode: Pressure Direction)

Mode: Threshold Threshold Condition: Lower or Equal | Mode: Threshold Threshold Condition: Equal | Mode: Pressure Direction Controller Pressure Rising: Controller 1 Controller Pressure Falling: Controller 2
Controller Selector changes when the Target Pressure is below a specified Threshold value If Target Pressure is lower than several Thresholds values, the lowest one is taken. If Target Pressure is higher than the highest Threshold, the highest one is taken. | Controller Selector changes only when the Target Pressure is equal to a Threshold value | Controller Selector changes depending on whether Target Pressure is rising or falling

Parameter:

Pressure Control.General Settings.Automated Controller Selector

Parameter | Description
--- | ---
Enable | Switches on/off the function
Mode | Threshold Pressure Direction
Controller Selector Bitmap | Used if Mode = Threshold Defines which controllers are automatically selected
Threshold Condition | Used if Mode = Threshold Lower or Equal Equal The Thresholds are related to Target Pressure
Controller 1 Threshold Controller 2 Threshold Controller 3 Threshold Controller 4 Threshold | Used if Mode = Threshold The Thresholds are related to Target Pressure
Controller Pressure Rising Controller Pressure Falling | Used if Mode = Pressure Direction Select one Controller for up control and one for down control Controller 1 Controller 2 Controller 3 Controller 4