# Extended Warnings - Bitmap description

Navigation: Valve Firmware > Interface > Profibus > Cyclic Buffers > Input Buffer > # Extended Warnings - Bitmap description |

Extended Warnings
Bit | Name | Description
0 | Remote Control Not Possible | Remote control not possible, access mode local is active, change to access mode remote or access mode locked
1 | Actual Control Mode Target Not Allowed | Not possible to switch the current control mode to given "Control Mode Target" because of reasons: • Actual Control mode is interlock or fatal error • Control Mode Target is 5 (pressure), 6 (hold) or 7 (learn) and no sensor is selected (sensor mode configuration)
2 | Zero Disabled | Using zero function not possible
3 | PFO Deactivated | Power Failure Option is deactivated
4 | Not Used | Reserved
5 | Out Of Range: Target Pressure | Target Pressure value is out of its defined range
6 | Out Of Range: Target Position | Target Position value is out of its defined range
7 | Not Used | Reserved
8 | Out Of Range Sensor 1 | Pressure Sensor 1 value is out of the defined range
9 | Out Of Range Sensor 2 | Pressure Sensor 2 value is out of the defined range
10 | Out Of Range Control Mode Target | Control Mode Target value is out of its defined range
11 | Out Of Range: General Control | General Control value is out of its defined range
12 | Not Used | Reserved
13 - 15 | Not Used | Reserved