# Connection

Navigation: Valve Firmware > Interface > DeviceNet > # Connection |

Connector type: Micro-style male (5 pin), connector is shown on panel refer to chapter Micro Connector Pinout.

At valve controller | DeviceNet® cable
PIN | Name | Wire color | Description
1 | Drain | Bare | Shield
2 | V+ | Red | DeviceNet® power supply +
3 | V- | Black | DeviceNet® power supply -
4 | CAN_H | White | DeviceNet® signal
5 | CAN_L | Blue | DeviceNet® signal

| The DeviceNet® interface is galvanically isolated from control unit.